DATED 4-9-2025

OLYMPIC PENINSULA ANTIQUE TRACTOR AND ENGINE ASSOCIATION

ATV/ UTV PULLING RULES

1. **Absolutely no consumption of alcoholic beverages until after your last pull of the day. Anyone found to have consumed any alcoholic beverage before their pull will be disqualified and not allowed to pull. Your pulling fees will not be refunded.**
2. A family membership qualifies one of the family members for a one time first free hook fee. All subsequent hooks by members of the same family will be charged the $15.00 fee for ATV/UTV pulls.
3. QUADS AND SIDE BY SIDE BY SIDES ARE ALLOWED. **NO 3 WHEELERS ALLOWED**
4. ALL VEHICLES WILL HAVE A CLEVIS, BALL HITCH THAT THE PULLING SLED CAN HOOK TO.
5. HITCH HEIGHT MUST NOT BE HIGHER THAN THE CENTER LINE OF THE REAR AXLE AND MUST NOT EXTEND NO FATHER THAN SIX INCHES FROM THE CENTER OF THE REAR AXLE.
6. NO SUSPENSION IS ALLOWED TO BE STRAPPED OR RATCHED DOWN.
7. EACH WEIGHT CLASS WILL INCLUDE THE WEIGHT OF THE MACHINE PLUS THE WEIGHT OF THE DRIVER.
8. ALL ATV’s MUST BE OPERATED IN A SAFE MANNER ON AND OFF THE TRACK. NO SPEEDING OR WHEELIES ALLOWED. THE SPEED LIMIT WHILE ON THE SHOW GROUNDS IS 5 MPH MAX.
9. ALL ENTRIES MUST STAY WITHIN THE PULL AREA UNTIL THEIR PULL IS COMPLETED. NO OTHER RIDING AROUND ON THE GROUNDS OR ON THE STREET IS ALLOWED. ONCE YOUR PULL IS COMPLETED, YOU MAY DRIVE YOUR UNIT DIRECTLY TO YOUR TRAILER.
10. ALL ATV’s MUST USE ONLY 2 REAR WHEELS. NO DUAL WHEELS ALLOWED.
11. ATV’S MUST HAVE WORKING BRAKES, FENDERS OVER THE TWO REAR TIRES AND A SPRING RETURN THROTTLE(LEVER OR TWIST).

11. ALL DRIVERS MUST WEAR A SHIRT, LONG PANTS, SHOES AND A HELMET DURING THE PULL.

12. THE FIRST PULLER IN EACH CLASS IS THE “TEST PULLER”. HE/SHE HAS THE OPTION TO REPULL IN THIRD OR LAST SPOT IN THAT CLASS. THE DECISION TO REPULL MUST BE MADE TO THE TRACK OFFICIAL BEFORE THE PULLER LEAVES THE TRACK.

13. IF THE ATV OR ANY PART OF THE SLED GOES OUT OF BOUNDS, THEY ARE AUTOMATICALLY DISQUALIFIED.

14. THE PULLER WILL HAVE TWO CONSECUTIVE ATTEMPTS TO START THE SLED MOVING. ONCE THE PULL HAS STARTED, THE PULL IS ENDED WHEN THE ENGINE STALLS OR FORWARD MOVEMENT HAS ENDED. NO JERKING OR HOLE DIGGING ALLOWED.

15. ALL PULLS WILL START WITH A TIGHT HITCH. NO JERKING IS ALLOWED.

16. ANYTHING THAT FALLS OFF OR OUT OF THE ATV/UTV DURING THE PULL WILL BE A DISQUALIFICATION.

17. THE STANDARD TRACK WILL BE 200 FEET LONG AND 25 FEET WIDE.

18. ALL ENTRIES WILL STOP ONCE THE FIRST ATV OF THAT CLASS HOOKED TO THE SLED.

19. ONLY PUMP GAS ALLOWED FOR USE AS A FUEL. NO ALCOHOL OR NITROUS WILL BE ALLOWED.

20. EACH PARTICIPANT IS ALLOWED ONLY ONE PULL PER WEIGHT CLASS EXCEPT IN THE CASE OF A TIE OR PULL OFF. IN THE EVENT OF A PULL OFF, AN ADDITIONAL HOOK FEE WILL NOT BE CHARGED

21. DRIVER MUST REMAIN SEATED DURING THE ENTIRE PULL.

22. DECISION OF THE JUDGES IS FINAL AND MUST BE ACCEPTED IN A SPORTSMANSHIP-LIKE MANNER.

23. THE ATV MAY BE RECHECKED AFTER THE PULL HAS ENDED IF THERE IS A QUESTION OF A RULE VIOLATION.

24. ONCE A PULLER BACKS UP TO THE SLED TO HOOKED, THE OPERATOR WILL TAKE THE ATV OUT OF GEAR, RELEASE THE CLUTCH AND EXTEND HIS ARMS OUTWARD. AT THE COMPLETION OF THE PULL, THE OPERATOR WILL BACK THE ATV UP TO UNHOOK THEN TAKE THE ATV OUT OF GEAR AND EXTEND HIS ARMS OUTWARD TO INDICATE TO PULLING STAFF THAT IT IS SAFE TO UNHOOK.